Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 20 - LIT-18626-12-95
P. 20

    General and important labels

           Other labels
             17
             Except for 252XE                   252XE

                MAXIMUM CAPACITIES                 MAXIMUM CAPACITIES
                12   PERSONS OR 2200   LBS.        12   PERSONS OR 2200   LBS.
                  2600 POUNDS, PERSONS, GEAR         2350 POUNDS, PERSONS, GEAR
             THIS BOAT COMPLIES WITH U.S. COAST GUARD SAFETY  THIS BOAT COMPLIES WITH U.S. COAST GUARD SAFETY
             STANDARDS IN EFFECT ON THE DATE OF CERTIFICATION  STANDARDS IN EFFECT ON THE DATE OF CERTIFICATION
             MEETS U.S. EPA EVAP STANDARDS USING CERTIFIED COMPONENTS  MEETS U.S. EPA EVAP STANDARDS USING CERTIFIED COMPONENTS
             MANUFACTURER:  YAMAHA JET BOAT MANUFACTURING U.S.A., INC.  MANUFACTURER:  YAMAHA JET BOAT MANUFACTURING U.S.A., INC.
             MODEL:                    VONORE, TN  MODEL:                 VONORE, TN
              DESIGN COMPLIANCE WITH NMMA REQUIREMENTS IS VERIFIED.  DESIGN COMPLIANCE WITH NMMA REQUIREMENTS IS VERIFIED.
               MANUFACTURER RESPONSIBLE FOR PRODUCTION CONTROL.  MANUFACTURER RESPONSIBLE FOR PRODUCTION CONTROL.
                        R                                  R
                          NATIONAL MARINE                    NATIONAL MARINE
                          MANUFACTURERS ASSOCIATION          MANUFACTURERS ASSOCIATION
             18                                 19

             20

               All applicable electrical system components installed as
               original equipment meet appropriate U.S.C.G. requirements
               for ignition protection. (Ref. 33 CFR 183.410 and 183.440)
               YAMAHA                     60E-83627-00

           12

| 15 16 17 18 19 20 21 22 23 24 25 |