Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 130 - LIT-18626-12-95
P. 130

    Equipment operation

           NOTICE                               To collapse the wakeboard tower:
                                                (1) 252XE: Fold the mirror. (See page 112 for
           Do not modify the wakeboard tower to tow  information on folding the mirror.)
           from it or to carry accessories not de-  (2) While an assistant supports the wake-
           signed for it. The wakeboard tower could  board tower, completely loosen the lock
           be damaged. Also, the wakeboard tower   knobs on both sides of the wakeboard
           collapsing feature is intended for storage  tower.
           only. The boat should not be transported
           or operated  with the tower  in the col-
                                                                       1
           lapsed position.                                                   2

           Collapsing and setting up the
           wakeboard tower
           (AR250 / 252S / 252XE)
           When storing  the boat, collapse the wake-
           board tower.
           NOTICE
                                                1  Wakeboard tower
           z Accidentally  dropping the wakeboard  2  Lock knob
            tower while collapsing or raising it can
            damage the tower, the boat, or both. An  (3) Lower the wakeboard  tower until it
            assistant needs to help hold the wake-  stops.
            board tower in place during the proce-
            dure.
           z Do not operate the boat or transport it
            on the trailer with the tower in the col-
            lapsed position to avoid possible dam-
            age.

                                                To set up the wakeboard tower:
                                                (1) Lift the wakeboard tower.
                                                (2) While an assistant supports the wake-
                                                   board tower, tighten the lock knobs on
                                                   both sides of the wakeboard tower until
                                                   they stop.

           122

| 125 126 127 128 129 130 131 132 133 134 135 |