Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 175 - LIT-18626-12-95
P. 175

    Operation

           (9) Reinstall the hull drain plug.  NOTICE:
              Tighten the hull drain  plug  securely
              before launching the boat. Otherwise,
              water may flood the boat and cause it
              to submerge. Clean any foreign mate-
              rial, such  as dirt or sand, from the
              threads  and the O-ring on the hull
              drain plug before installing the drain
              plug.
           (10) Spray a rust inhibitor, such as Yamaha
              Silicone Protectant and Lubricant, on
              metallic parts to minimize corrosion.
           (11) Use a boat cover designed for your boat,
              or store the boat in a building or under a
              canopy or carport in order to prevent rain
              from falling onto the boat. Because all of
              the water  will not be drained from  the
              deck automatically, take sufficient mea-
              sures to prevent rainwater from entering
              the boat. NOTICE: Make sure that the
              turnbuckles on the boat cover do not
              contact the boat directly when using
              the cover. Otherwise, the boat could
              be damaged.
           (12) Turn the battery switch to the OFF (red)
              position. (See page 37 for more informa-
              tion.)

                                                                                167

| 170 171 172 173 174 175 176 177 178 179 180 |