Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 136 - LIT-18626-12-95
P. 136

    Equipment operation

             Bimini top (252SE / 252SD)
           Removing the bimini top
           To remove the bimini top:
           (1) Open both flaps on each side of the bimi-              1
              ni top.

                                                         2

                                                1  Buckle
                                                2  Flap
                       1                        (4) Slowly pull the bimini top toward the bow
                                                   and remove it.
           1  Flap
                                                Installing the bimini top
           (2) Loosen the ratchet, and then loosen the  To install the bimini top:
              strap securing the bimini top.    When installing the bimini top, simply reverse
                                                the removal steps.

                      1

                2

           1  Ratchet
           2  Flap
           (3) Open the flaps at the front and rear of the
              bimini top and release the buckles.

           128

| 131 132 133 134 135 136 137 138 139 140 141 |