Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 120 - LIT-18626-12-95
P. 120

    Equipment operation

                      Windshield                To adjust the mirror angle:
           The windshield can be opened and closed.  Loosen the upper lock knob, adjust the angle
                                                of the mirror, and then tighten the knob.
               WARNING
           To avoid injury, the windshield must be se-
                                                        1
           cured when the boat is in motion.
           To close the windshield:
           To  close the windshield, Close the wind-
           shield, and then turn the windshield latches
           to the lock position.

                                                1  Upper lock knob

                                                To fold the mirror:
                  1
                                                Loosen the lower lock knob, fold the mirror,
                                                and then tighten the knob.

           1  Windshield latch
                                                     1
           To open the windshield, turn the windshield
           latches to the unlock position, and then open
           the windshield.

           Folding mirror (252XE)
           The mirror is installed on the driver’s side of
           the windshield.                      1  Lower lock knob

                                       1

           1  Folding mirror

           112

| 115 116 117 118 119 120 121 122 123 124 125 |