Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 81 - LIT-18626-12-95
P. 81

    Instrument operation

                                                       Operation buttons
                                                In addition to touching the multi-function dis-
                                                play directly, you can use the operation but-
                           VOLUME
                           (SCROLL)
                        HOME   CANCEL           tons and the controller to operate  various
                                                functions.
                                                Controller
                         CRUISE  CRUISE
                         NO WAKE  NO WAKE
                                                              1  2 3
                                                                 VOLUME
                                                                 (SCROLL)
                                                             HOME   CANCEL
           TIP:
           Although the procedures in this manual ex-
           plain how to make selections by touching the
           display, you can also make selections using         CRUISE  CRUISE
                                                                   NO WAKE
                                                               NO WAKE
           the joystick knob.
                                                               4   5
                                                        Name           Function
                                                 1  “HOME” button  Displays the home
                                                                  screen. (See page 80.)
                                                 2  “VOLUME  –    Switches the joystick
                                                    (SCROLL)” but-  between the volume
                                                    ton           control mode and the
                                                                  navigation control
                                                                  mode. When the main
                                                                  switches are turned to
                                                                  the on position, the
                                                                  volume control mode
                                                                  is selected by default.
                                                 3  “CANCEL” but-  Deselects the current-
                                                    ton           ly selected item.
                                                 4  “CRUISE/NO    Activate and set the
                                                    WAKE” (–) but-  cruise assist, no-wake
                                                    ton           mode, and reverse
                                                 5  “CRUISE/NO    RPM control. (See the
                                                    WAKE” (+) but-  following sections.)
                                                    ton

                                                Operating the boat at a steady speed
                                                (cruise assist)
                                                The cruise assist feature is for steady engine
                                                speed operation when the boat is traveling
                                                above no-wake speeds. The cruise assist is
                                                available for use whenever the engines are

                                                                                 73

| 76 77 78 79 80 81 82 83 84 85 86 |