Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 143 - LIT-18626-12-95
P. 143

    Operation and handling requirements

           (5) Stop filling when the fuel just becomes  Engine oil requirement
              visible in the bottom of the filler tube. Do  Engine oil
              not “top off” the tank, because gasoline  NOTICE
              could spill out.
           (6) Wipe up any spilled fuel immediately.  Use only 4-stroke engine oil. Usage of 2-
           (7) Close the fuel tank filler cap by pushing it  stroke engine oil could result in severe en-
              until it locks in place. Make sure that the  gine damage.
              fuel tank filler cap is securely closed.
                                                Select an oil grade according to the average
           Engine Med RX Fuel Additive
           As the fuel mixture burns in your engine’s  temperatures in the area where the boat will
                                                be used.
           combustion chambers, carbon deposits are
           left behind. Over time, these deposits can re-  Recommended engine oil:
           duce performance  and even  cause engine  YAMALUBE 4W
           damage. Marine engines tend to run at lower  Recommended engine oil type:
           operating temperatures than other engines,  SAE 10W-30, 10W-40, 20W-40, 20W-
           making them more likely to accumulate these  50
           harmful deposits. Engine Med RX, available  Recommended engine oil grade
           from your Yamaha Boat Dealer, is formulated  (3-star models):
           to remove existing deposits and, when used  API SG,SH,SJ,SL
           continuously, prevent new ones from form-  Recommended engine oil grade
           ing, while also helping to keep fuel injectors  (4-star models):
           and other fuel system components clean for  API SJ,SL
           proper performance and longer engine life.
                                                3-star models

                                                                                135

| 138 139 140 141 142 143 144 145 146 147 148 |