Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 155 - LIT-18626-12-95
P. 155

    Pre-operation checks

           Engine oil level check               4-star models
           Make sure that the engine oil level is between
           the minimum level mark and maximum level
           mark on the dipstick. (See page 136 for infor-         1
           mation on checking the engine oil level.)
           3-star models

                           1

                                                1  Dipstick

           1  Dipstick
                                                                         1
                                                                           2

                                  1
                                     2

                                                1  Maximum level mark
                                                2  Minimum level mark

           1  Maximum level mark
           2  Minimum level mark

                                                                                147

| 150 151 152 153 154 155 156 157 158 159 160 |