Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 190 - LIT-18626-12-95
P. 190

    Maintenance

                                                         Initial   Thereafter every
                                                                 50     100   200
                  Item                 Operation           10   hours   hours   hours
                                                         hours  or 12   or 12   or 24
                                                               months  months  months
                                                                 *1     *1     *1
           Steering master    Check operation and tilting mecha-  √      √
           ASSY               nism, and check for looseness
                              Check hydraulic fluid level, and
           Steering system    check for dirt in fluid
           (hydraulic system)   Check for hydraulic fluid leakage,   √   √
           (252SD)            and check parts for wear and dam-
                              age
                              Check operation from steering mas-
           Steering system    ter ASSY to jet thrust nozzles, and   √    √
           (252SD)            check for free play
                              Check jet pumps for corrosion
           Steering system    Check connections of connectors,
           (electrical system)   and check for looseness   √             √
           (252SD)
           Steering cables    Check connections and exterior,            √
           (except for 252SD)  and lubricate
           Throttle/shift pad-  Check operation            √             √
           dles (252SD)
                              Check operation, and check link rod
           Articulating keel                                             √
                              for bends and damage
                              Check exterior and operation,
           Remote control le-  check shift operation, and check for   √  √
           vers
                              looseness
           Throttle cables    Check connections and exterior,
           (AR250 / SX250 /   and lubricate                              √
           252S)
                              Check connections and exterior,
           Shift cables                                                  √
                              and lubricate (shift gate end)
           Exhaust hoses, wa-  Check for exhaust leakage, and
           ter locks, and resona-  check clamps at connections           √
           tors
           Drain passages     Remove clogs                               √
           Drain plug         Check O-ring                 √             √
           Hull and deck      Check for damage             √             √
                              Check installation and operation,
           Windshield and seats                            √             √
                              and check for damage
           Wakeboard tower    Check installation, and check for
           (except for SX250)   damage                     √             √
           and bimini top

           182

| 185 186 187 188 189 190 191 192 193 194 195 |