Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 161 - LIT-18626-12-95
P. 161

    Pre-operation checks

           252SE / 252XE / 252SD                es. If water is not flowing out of the pilot
                                                outlets during operation, do not continue
                                                to run the engines. Overheating and seri-
                                                ous damage could occur. (See “Over tem-
                                      1
                                                perature warning” on pages 68 and 96 for
                                                more information.)
                                      2
                                                Fuel level check
                                                Check the amount of fuel remaining in the
                                                fuel tank using the fuel level bar graph on the
                                                multi-function display.
           1  Engine shut-off switch
                                                AR250 / SX250
           2  Clip
           Cooling water pilot outlet check
                                                                 NW     N      NE
           Check that water comes out from the pilot  FUEL
           outlets while the engines are running in the  50  %      FLOAT MODE
           water. If water is not circulating, something  1
           may be clogging the intake grates. Refer to                      °F
           “Jet pump clean-out procedure” on page                    Water Temp
           190.                                          START
                                                        36.3  V
                                                        Bilge  Blower            Nav
                                                1  Fuel level bar graph
                                                252S / 252SE / 252XE / 252SD
                                                   1

                                                                      SE    S
                                                  FUEL
                                                  100 %
                                                      19
           TIP:                                              x1000 rpm
           It  may take up to 20 seconds for water  to                     MPH
           reach the pilot outlets when  first launching  13.0  V  9
                                                     START
           the boat. The amount and force of the exiting      Bilge  Blower
           water will vary with engine speed.   1  Fuel level bar graph
           NOTICE
                                                Add fuel if necessary. (See page 134 for infor-
           A continuous flow of water from the pilot  mation on filling the fuel tank.)
           outlets shows  that water is  flowing
           through the engine cooling water passag-

                                                                                153

| 156 157 158 159 160 161 162 163 164 165 166 |