Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 57 - LIT-18626-12-95
P. 57

    Instrument operation

           z While the cruise assist is activated, the en-  The no-wake mode can be set to 3 engine
            gine speed can also be adjusted by operat-  speeds. To adjust the engine speed while the
            ing the remote control levers.      no-wake  mode is activated, push the
                                                “CRUISE/NO   WAKE”   (+)  button  or
           To deactivate the cruise assist:     “CRUISE/NO WAKE” (–) button.
           Operate the remote control  levers  to de-  To deactivate the no-wake mode:
           crease the engine speed to 3000 rpm or less.  Perform one of the following operations.
           When “Cruise” and the cruise assist setting  z Push  the “CRUISE/NO WAKE” (–) button
           level disappear, the cruise assist is deactivat-  repeatedly until “No Wake” disappears.
           ed.                                  z Push the remote control levers forward to
                                                  open the throttle.
           Operating the boat with a minimal
           wake (no-wake mode)                  Operating the boat in reverse with
           The no-wake mode is useful for operating the  more thrust (reverse RPM control)
           boat at a steady speed with a minimal wake.  Engine speed in reverse is limited to approx-
           This is especially convenient when traveling  imately 4500 rpm. If more thrust is required
           in harbors, channels, or other areas posted  when the boat is traveling in reverse, use the
           with low speed limits as “no wake zones”.  reverse RPM control.  WARNING! Be  pre-
           The no-wake mode can be used only when  pared to  reduce throttle as  soon as the
           the engines are operating at idle speed.  boat moves as desired.  Otherwise, the
           To activate the no-wake mode:        boat may become unstable, which could
           (1) Put the remote control levers in the TDE  result in loss of control and an accident.
              position or forward position so that both  To activate the reverse RPM control:
              engines are operating at idle speed.  (1) Move the remote control levers  back-
           (2) Push the  “CRUISE/NO WAKE” (+) but-  ward so that the throttle is opened in re-
              ton. When the no-wake mode is activat-  verse and both engines are operating at
              ed, “No Wake” will be displayed under  the same engine speed.
              the boat speed.                   (2) Increase the engine speed to 4500 rpm,
                                                   and then push the “CRUISE/NO WAKE”
                    SE      S      SW
                                                   (+) button.
                                                Once the reverse RPM control is activated,
                                                pushing the “CRUISE/NO WAKE” (+) button
                                                will increase the  available  engine speed by
                                                approximately 500 rpm in 3 stages up to a
                           MPH                  maximum of 6000 rpm, and pushing the
                          No Wake               “CRUISE/NO WAKE” (–) button will decrease
                                                the available engine speed. However, the ad-
                            1                   justment is limited to these 3 increments.
           1  “No Wake”

                                                                                 49

| 52 53 54 55 56 57 58 59 60 61 62 |