Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 205 - LIT-18626-12-95
P. 205

    Trouble recovery

                              2 3 4 5             Fuse amperage:
                                                    Electronic throttle valve fuse:
                                                      10 A
                              9  8  7  6            Fuel pump fuse:
                                                      10 A
                                                    Main relay drive fuse:
                                                      10 A
                                  1
                                                    Main fuse:
                                                      20 A
                                                    Battery fuse (AR250 / SX250 / 252S):
           1  Accessory fuse cover
                                                      30 A
           2  Display/Buzzer/GPS/Audio Controller/
             Switch Panel fuse                      BCU fuse:
                                                      50 A (252SE / 252XE / 252SD)
           3  CLH/CLG/Power Port/USB fuse
           4  Horn fuse                             Display/Buzzer/GPS/Audio Controller/
           5  Bilge pump fuse                       Switch Panel fuse:
           6  Power distribution module fuse          20 A
           7  USB fuse                              CLH/CLG/Power Port/USB fuse:
           8  Accessory 2 fuse                        20 A
           9  Accessory 1 fuse                      Horn fuse:
                                                      7.5 A
           (5) Replace the blown fuse with the spare
                                                    Bilge pump fuse:
              fuse of the correct amperage by using
                                                      3 A
              the fuse puller.
                                                    Power distribution module fuse:
                                                      20 A
                                                    USB fuse:
                                                      3 A
                                                    Accessory 1 fuse:
                                                      20 A
                                                    Accessory 2 fuse:
                                                      20 A

                                                (6) Install the fuse box cover.
                                                (7) If an accessory fuse was replaced, install
                                                   the accessory fuse holder or cover.
                                                (8) Close the engine hood.

                                                                                197

| 200 201 202 203 204 205 206 207 208 209 210 |