Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 199 - LIT-18626-12-95
P. 199

    Trouble recovery

                     1

                                                                            1

                                                       3
                                                                           2

           1  Access port cap                   1  “SET” mark
                                                2  Slot
           (5) Remove any weeds or debris from the  3  Edge of the access port
              drive shaft, impeller, pump housing, and
              jet thrust nozzle. If you cannot remove  (8) Check that the cap is perpendicular to
              the debris, consult a Yamaha Boat Deal-  the centerline of the boat. Pull the handle
              er.                                  forcefully  to make sure  that the cap is
           (6) To reinstall the access port  cap, first  locked securely. If a strong pull will move
              clean off any sand or other foreign matter  the access port cap, it is not locked se-
              from the cap or port surfaces. Apply a  curely—the cap could be forced out by
              light coat of Yamalube Waterproof Ma-  water pressure during operation.
              rine Grease (P/N: ACC-GREAS-10-CT), if
              available, to the seal of the access port
              cap. If grease is not available, apply the
              grease  during  the  post-operation
              checks.                                1
           (7) Insert the cap so that the “SET” mark is
              aligned  with  the slot, and then while
              pushing the handle turn the cap clock-
              wise until the “SET” mark is aligned with
              the edge of the access port.
                                                1  Perpendicular to the centerline of the boat

                                                (9) Close the rear platform hatch.
                                                 NOTICE

                                                Be sure the access port caps are locked
                                                securely in place. Otherwise, the caps
                                                could be forced out of the access ports by
                                                water pressure,  causing loss of  perfor-
                                                mance and possible damage.

                                                                                191

| 194 195 196 197 198 199 200 201 202 203 204 |