Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 127 - LIT-18626-12-95
P. 127

    Equipment operation

                                                     Remote control keypad
                                                The remote control keypad is located on the
                                                starboard side of the swim platform.
                                                For operating instructions, refer to the stereo
                 2
                                   1            system owner’s manual included with your
                                                boat.

                                                                               1

           1  Swim platform shower handle
           2  Flow control button

           TIP:
           The  shower can provide up to 5.3 L
           (1.4 US gal, 1.2 Imp.gal) per minute flow
           through the retractable shower handle.
                                                1  Remote control keypad
           (4) Feed the shower handle hose back into
              the opening and place the swim platform
              shower handle in its cradle.
           (5) Close the swim platform shower cover.
           (6) Tap the “Shower” button to select the
              “Shower” button on the system control
              screen to turn the shower pump off.

                                                                                119

| 122 123 124 125 126 127 128 129 130 131 132 |