Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 186 - LIT-18626-12-95
P. 186

    Care and storage

           z Pivot points
           Grease all pivot points  of the  steering and  1
           shift mechanisms at the pump ends.

                                                1  Bearing housing grease nipple

           z Bearing housings
           Grease  the bearing housings through the
           grease nipples.  NOTICE: Fill the grease
           slowly and carefully, because it can dam-
           age the hoses and the joints.
           The  first service should be  done after 10
           hours or 1 month by a Yamaha Boat Dealer.
           Fill the bearing housings with water-resistant
           grease through the grease nipples.
             Grease capacity:
               33.0–35.0 cc (1.11–1.18 oz)

           After  first service:  Every  100 hours or 6
           months (you may do this yourself).

             Grease capacity:
               6.0–8.0 cc (0.20–0.27 oz)

           178

| 181 182 183 184 185 186 187 188 189 190 191 |