Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 19 - LIT-18626-12-95
P. 19

    General and important labels

            13                                   14

             15
             AR250/252S/252SE/252SD/252XE

             16
             252XE

              Improper use of the ballast system can
              overload the boat, causing poor handling and
              increased risk of swamping.
              Ballast system adds 1685 lb (764 kg) when full.
              Include this weight when making sure your
              load does not exceed the weight shown on
              the Maximum Capacities Label.

              Drain ballast completely before trailering the
              boat to reduce the risk of a towing accident.
              The Increased weight of ballast can cause
              unsafe towing conditions due to negative
              tongue weight, including decreased tow
              vehicle stability and greater chance of a
              runaway trailer that has come off the hitch.

                                                                                 11

| 14 15 16 17 18 19 20 21 22 23 24 |