Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 163 - LIT-18626-12-95
P. 163

    Operation

            operate the blowers if  you can  smell  drain plug and make sure that the plug is
            gasoline vapors in the engine compart-  tightened securely  before launching the
            ment or if there are any loose electrical  boat. Otherwise, water may flood the boat
            connections. Contact a  Yamaha Boat  and cause it to submerge.
            Dealer if there is a problem you cannot
            locate or correct.
           z Attach the engine shut-off cord (lanyard)
            to your PFD before operating. Failure to
            attach the cord could  result in a run-
            away boat if the operator is ejected.
           z Do not apply throttle when anyone is at
            the rear of the boat. Turn the engines off
            or keep them at idle. Water and debris
            exiting the jet thrust nozzles can cause
                                                                          1
            severe injury.
                                                1  Hull drain plug
           (1) Always make sure the boat is launched
              and used in waters that are free from  (2) Turn the battery switch to the ON posi-
              weeds and  debris,  and at least 90 cm  tion.
              (3 ft) deep from the bottom of the boat.  (3) Turn the main switch keys to the on po-
              WARNING! Never operate in water      sition to operate the blowers automati-
              that is less than 90 cm (3 ft) deep from  cally for 5 minutes.
              the bottom of the boat. You increase  TIP:
              your chance of hitting an underwater  To operate the blowers manually, tap the
              obstacle. You could be injured. Peb-  “Blower” button. Ventilate the engine com-
              bles or sand can also be sucked into  partment for at least 4 minutes, and then tap
              the  jet intakes,  damaging the impel-  the “Blower” button again  to turn  off the
              lers.                             blowers.

                                                            NW    N    NE
                                                   FUEL                        DEPTH
                                                  50  %       FLOAT MODE       0  Ft
                                                                     °F
                        90 cm (3 ft)
                                                               Water Temp
                                                     START                   HOUSE
                                                    36.3  V                  11.8  V
                                                    Bilge  Blower        Nav  Anchor
                                                         1
           NOTICE                               1  “Blower” button
           There is a hull drain plug at the bottom of
           the  stern. Check the O-ring on  the  hull

                                                                                155

| 158 159 160 161 162 163 164 165 166 167 168 |