Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 158 - LIT-18626-12-95
P. 158

    Pre-operation checks

           252SE / 252SD                        AR250
                                                           2
                                                                              1
                                      1

           1  “BLOWER” switch                   1  Bow light
                                                2  Anchor light
           Navigation and anchor lights checks
           Make sure that the bow light and anchor light  SX250
           operate properly.
           The procedure for setting up the anchor light    2
           varies according to the model. See the page
           indicated below for your boat.                                 1
           SX250: See page 114.
           TIP:
           SX250: Before operating the boat in daylight
           hours after checking the navigation and an-
           chor lights, store the anchor light.
           252S / 252SE / 252XE / 252SD
                                                1  Bow light
                              2                 2  Anchor light

                                          1     To check the operation using the multi-func-
                                                tion display:
                                                (1) Tap the “Navigation” light button on the
                                                   system control screen. Check that the
                                                   bow light and anchor light come on when
                                                   the button is blue and that both lights go
                                                   off when the button is gray.
                                                (2) Tap the “Anchor” light button on the sys-
           1  Bow light
                                                   tem control screen. Check that only the
           2  Anchor light
                                                   anchor light comes on when the button is
                                                   blue and that the anchor light goes off
                                                   when the button is gray.

           150

| 153 154 155 156 157 158 159 160 161 162 163 |