Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 123 - LIT-18626-12-95
P. 123

    Equipment operation

           (3) Open the cap of the anchor light socket,    Bow ladder
              fit the protrusion on the anchor light into  The bow ladder is located in the anchor stor-
              the slot in the socket, and then install the  age compartment.
              light into the socket.

                                           3         2
                                                                           1

                                                                             3

             1                            2
                                                1  Bow ladder
           1  Cap                               2  Bow ladder strap
           2  Slot                              3  Anchor storage compartment
           3  Protrusion
                                                To use the bow ladder:
           (4) Fit the anchor light stopper into the an-  (1) Open the anchor storage compartment
              chor light socket.                   lid. (See page 103.)
                                                (2) Slide the bow ladder toward the bow.
                                                (3) Extend the bow ladder, and then flip the
                                           1       ladder forward and lower it.
                                                (4) Close the anchor storage compartment
                                                   lid to use it as a step.

                                                                              1
           1  Anchor light stopper
           To store the anchor light:
           (1) Pull the anchor light stopper upward, re-
              move the anchor light, and then close the
              cap of the anchor light socket.
                                                1  Bow ladder
           (2) Install  the  anchor light into the  anchor
              light holder, and then close the ski lock-
              er.

                                                                                115

| 118 119 120 121 122 123 124 125 126 127 128 |