Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 134 - LIT-18626-12-95
P. 134

    Equipment operation

           Storing the bimini top               (3) Push the snap button and shorten each
           To store the bimini top:                rear support pole to the short position.
           (1) While pulling the main pole down slightly,
              push the snap button, and then extend
              each rear support pole to the long posi-  1
              tion to loosen the bimini top.
                                                        2

                   1
                                                        3
                   2

                                                1  Rear support pole
                   3                            2  Short position
                                                3  Snap button

           1  Rear support pole                  NOTICE
           2  Snap button
                                                Be careful not to push the snap button and
           3  Long position
                                                extend the  pole too far. Otherwise,  the
           (2) Remove each rear support pole from the  lower section of the pole could fall into the
              rear support pole mounting bracket by  water.
              rotating the lock pin.
                                                (4) Hook the rear support poles  onto the
                                                   main pole, and then pull the rear of the
                                     1
                                                   bimini top toward the bow.

                         2         3

                                                                      2

                                                   1

           1  Rear support pole
           2  Lock pin
           3  Rear support pole mounting bracket
                                                1  Rear support pole
                                                2  Main pole

           126

| 129 130 131 132 133 134 135 136 137 138 139 |