Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 118 - LIT-18626-12-95
P. 118

    Equipment operation

                                                                                 1

                                                1  Wet storage compartment
           To fold the galley table:
           When installing the engine cover, simply re-  To close the wet storage compartment:
           verse the steps for extension.       (1) Close the rear platform hatch.
                                                (2) Turn the lock handles counterclockwise
           Wet storage compartment                 and make sure that the hatch is securely
           The wet storage compartment is located un-  closed.
           der the swim platform.               (3) Push the lock handles down.
           To open the wet storage compartment:  TIP:
           (1) Pull the lock handles up.        z The engines will not start if the rear plat-
           TIP:                                   form hatch is not securely closed.
           252S / 252SE / 252SD: The lock handles are  z 252S / 252SE / 252SD: Snap the buttons
           located under the swim platform seats.  on the bottom of each swim platform seat
           (2) Turn  the lock handles  clockwise, and  onto the button bases.
              then open the rear platform hatch.
                                                Stern storage compartments
                                  1             The stern storage compartments are located
                                                behind the swim platform seat backrests.
                                                To open a stern storage compartment, pull
                                                the strap on the swim platform seat backrest.

                                   2

           1  Rear platform hatch
           2  Lock handle

           110

| 113 114 115 116 117 118 119 120 121 122 123 |