Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 66 - LIT-18626-12-95
P. 66

    Instrument operation

                Item            Function        Chart Setup
           EDIT          Changes the name of, or   Perform settings for functions displayed on
                         deletes, the track.    the map.
           Show / Hide   Shows the track on the
                         map. Hide will make that
                         track invisible.                     Chart Setup
           Close         Returns to the Track Man-
                         ager screen.                  SHOW GRIDS     SHOW  TRACKS

                                                       SHOW TEXT      SHOW NAV AIDS
           Satellite status
           Display detectable satellites.              SHOW WAYPOINTS  SHOW WAYPOINT NAMES

                                                    Close
                  Satallite Status  N
               SATELLITES     3
               9:47
               Latitude:  35.6060
               Longitude:  -84.2541
               Op Mode:  0.00  W         E      To perform settings, select the item you want
               HDOP:  0.00
               VDOP:  0.00                      to display.
               TDOP:  0.00
               SOG:  0.0
               COG:  0
                                  S
              Close

           Depth / Position
           Perform  settings  for contour lines and  safe
           depths.

                        Depth / Position

               DEPTH CONTOUR
                 All  66ft  33ft  16ft  6ft  0ft
               SAFETY CONTOUR
                 66ft  33ft  16ft  6ft  0ft

              Close

           To perform settings, select the desired depth.
           Set depths are reflected on the map.

           58

| 61 62 63 64 65 66 67 68 69 70 71 |