Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 128 - LIT-18626-12-95
P. 128

    Equipment operation

           Side table
                                                                                1
               WARNING
           If  the side table is installed at the swim
           platform, do not use the table while the en-
           gines are running. Exhaust gases coming
           from underneath the swim platform con-
           tain carbon monoxide, a colorless, odor-
           less gas which may cause brain damage
           or death when inhaled. Symptoms include
           nausea, dizziness, and drowsiness.
                                                1  Side table
           NOTICE
                                                To install the side table, slide the end of the
           If  the side table is installed at the swim  table pole into  the  table bracket until it  is
           platform, remove the side table before op-  locked in place.
           erating the boat. Otherwise, the side table
           may fall into the water.

           The side table can be installed at the swim
           platform.

                                                 3
                1                                                         2
                                                                1
                                                1  Table bracket
                                                2  Table pole
                                                3  Table bracket knob

                                                To remove the side table, pull the table brack-
           1  Side table                        et knob, and then pull the table pole upward.

           AR250 / SX250: This model can also be in-
           stalled to the rearward of the driver’s seat.

           120

| 123 124 125 126 127 128 129 130 131 132 133 |