Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 96 - LIT-18626-12-95
P. 96

    Instrument operation

           To connect an external device:
           (1) Tap the “  ” button, and then select
              “+Add Device”.
           (2) Turn on the Bluetooth function of the ex-
              ternal device, and  then search for  the
              multi-function display unit of the boat.
                                                                               1
           TIP:
           Make sure that other external devices have
           their Bluetooth function disabled before be-                 5V
           ginning the pairing  process to reduce  con-
           nection issues.                      1  Auxiliary input jack

           (3) Tap the “Connect” button, and the “Con-  TIP:
              firm Pairing on  Device”  screen is dis-  z You can adjust the volume level of  the
              played.                             speakers using the multi-function display
           (4) Select “OK” for both the multi-function  unit or the volume control of the external
              display unit and the external device.  device.
                                                z To select the audio tracks, use the external
           To disconnect an external device, turn off the  device.
           Bluetooth function of the external device.
                                                Zone control screen
           Auxiliary screen                     Perform volume adjustment for each zone.
           Portable media players  and other external
           devices can be connected to the audio sys-
                                                              Zone Control
           tem to listen to the audio tracks stored on the
           devices through the audio system’s speak-
           ers.

                          Auxiliary

                                                    Back    Selected Zone: Interior

                                                To adjust the volume:
                                                (1) Tap the highlighted part.
              Source           MPH    Zone Control  (2) Adjust by moving the slider control to the
                                                   left or right.
                                                (3) Tap “Back”.
                                                TIP:
                                                Zones that can be set differ depending on the
                                                specifications.

           88

| 91 92 93 94 95 96 97 98 99 100 101 |