Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 70 - LIT-18626-12-95
P. 70

    Instrument operation

           (3) Tap the “Connect” button, and the “Con-  unit or the volume control of the external
              firm Pairing on  Device”  screen is dis-  device.
              played.                           z To select the audio tracks, use the external
           (4) Select “OK” for both the multi-function  device.
              display unit and the external device.
                                                Zone control screen
           To disconnect an external device, turn off the  Perform volume adjustment for each zone.
           Bluetooth function of the external device.

                                                              Zone Control
           Auxiliary screen
           Portable media players  and other external
           devices can be connected to the audio sys-
           tem to listen to the audio tracks stored on the
           devices through the audio system’s speak-
           ers.
                                                    Back    Selected Zone: Interior
                          Auxiliary

                                                To adjust the volume:
                                                (1) Tap the highlighted part.
                                                (2) Adjust by moving the slider control to the
                                                   left or right.
                                                (3) Tap “Back”.
                               MPH
              Source                  Zone Control
                                                TIP:
                                                Zones that can be set differ depending on the
                                                specifications.

                                          1

           1  Auxiliary input jack

           TIP:
           z You can adjust the volume level of the
            speakers using  the multi-function  display

           62

| 65 66 67 68 69 70 71 72 73 74 75 |