Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 64 - LIT-18626-12-95
P. 64

    Instrument operation

           Waypoint
           Set a waypoint for a destination on the map.    Waypoint Manager
           Waypoints can be attached to any location.
                                                          GR8            EDIT
           The “Add Waypoint” screen  is  displayed
           when a waypoint is attached.
                                                         Lat:        26.9484
                                                         Lon:        -80.0968
                       Waypoint Manager
                                                         Distance:    204.39  m
               GR8
                                                   Close   Delete    View    GoTo

                                                     Item            Function
                                                              Changes the color of the
                                                              waypoint.
              Close                   Add Waypoit  View       Views the waypoint on the
                                                              map.
                                                 GoTo         Provides the distance to the
                                                              waypoint, along with the
           To add a Waypoint:                                 latitude and longitude. It
           (1) Display the location you want to attach a      also tells when you have ar-
              waypoint to on the map.                         rived at the waypoint and
                                                              asks if you would like to
           (2) Tap “  ”.                                      stop the navigation.
           (3) Switch  to the “Add Waypoint”  screen,  Delete  Deletes the waypoint.
              and select any letters.            EDIT         Changes the name of the
                                                              waypoint.

                                                Cruising to the destination:
                                                (1) Select the waypoint created on the map.
                                                (2) Tap “GOTO”.
                        1
                               2
                                                        BAY
                 NEXT WAYPOINT 1.7 km
                     29°
                                                         Distance:  12.06
                              MPH
                                                         Lat: 45.28001
                                      REC
                                                         Lon: -92.97718
           (4) Tap “Save”.
           When the waypoint is set, “Waypoint Manag-
           er” is displayed, and the latitude and longi-
                                                          Delete     Edit
           tude of the set waypoint are displayed along
           with the distance from the current location.
                                                TIP:
                                                To stop tracking, tap “STOP”.

           56

| 59 60 61 62 63 64 65 66 67 68 69 |