Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 148 - LIT-18626-12-95
P. 148

    Operation and handling requirements

           z The bilge pump will operate every 2 min-
            utes automatically, even if the “Bilge” but-
            ton is not tapped.

           Even if the “Bilge” button is not tapped to op-
           erate the bilge pump, the bilge pump will de-
           tect when there is excessive water in the bilge
           and will automatically drain most of it through
           the bilge pump outlet. This  function works
           automatically, even if the battery switches are
           turned to the off position.
           TIP:
           When the bilge pump operates automatically,
           the bilge pump will not stop until most of the
           bilge water is drained.

           140

| 143 144 145 146 147 148 149 150 151 152 153 |