Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 12 - LIT-18626-12-95
P. 12

    General and important labels

                                                Two Stars - Very Low Emission
                                                The two-star label  identifies engines  that
                      1                         meet the Air Resources Board’s Personal
                                                Watercraft and Outboard marine engine 2004
                                                exhaust emission standards. Engines meet-
                                                ing these standards have 20% lower emis-
                                                sions than One Star-Low Emission engines.

           1  Star label location
           One Star - Low Emission
           The one-star label identifies engines that
           meet the Air Resources Board’s Personal
           Watercraft and Outboard marine engine 2001
           exhaust emission standards. Engines meet-
           ing these standards have 75% lower emis-
           sions than conventional carbureted two-  Three Stars - Ultra Low Emission
           stroke engines. These engines are equivalent  The three-star label identifies engines that
           to the U.S. EPA’s 2006 standards for marine  meet the Air Resources Board’s Personal
           engines.                             Watercraft and Outboard marine engine 2008
                                                exhaust emission standards or the Sterndrive
                                                and Inboard marine engine 2003-2008 ex-
                                                haust emission standards. Engines meeting
                                                these standards have 65% lower emissions
                                                than One Star-Low Emission engines.

           4

| 7 8 9 10 11 12 13 14 15 16 17 |