Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 10 - LIT-18626-12-95
P. 10

    General and important labels

           Port side                             Emission control information
                                                These engines conform to U.S. Environmen-
                                                tal Protection Agency (EPA) and/or California
                                                Air Resources Board (CARB) regulations for
              YAMAHA                            marine SI engines applicable at the time of
                                                manufacture.
                                                The 4-star labels are affixed to models that
                                                meet the  Air Resources  Board’s emission
              YAMAHA MOTOR CO., LTD.
              MADE IN JAPAN                     standards for 4-star models. (See page 3 for
              PAYS D’ORIGINE JAPON              information on the star labels.)
                                                Star labels are not affixed to 3-star models.
                                                These engines are certified to operate on reg-
                                                ular unleaded gasoline.

           Starboard side                       Approval labels of emission control
                                                certificate
                                                These labels are attached to each engine unit
                                                and to the inside of the engine compartment.
                                                (See page 103 for engine hood opening and
              YAMAHA                            closing procedures and page 179 for engine
                                                cover removal and installation procedures.)

              YAMAHA MOTOR CO., LTD.                            1
              MADE IN JAPAN
              PAYS D’ORIGINE JAPON

                                                1  Emission control information label

                                                3-star models

                                                 EMISSION CONTROL INFORMATION
                                                 THIS ENGINE CONFORMS TO          U.S. EPA EXHAUST REGULATIONS FOR SI MARINE
                                                 ENGINES. REFER TO OWNER’S MANUAL FOR MAINTENANCE SPECIFICATIONS AND
                                                 ADJUSTMENTS.
                                                  ENGINE FAMILY :  DISPLACEMENT :                                            liters
                                                  MAX POWER :                                    kW  EPA FEL : HC+NOx               , CO                g/kW-h
                                                 YAMAHA MOTOR CO.,LTD.

           2

| 5 6 7 8 9 10 11 12 13 14 15 |