Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 69 - LIT-18626-12-95
P. 69

    Instrument operation

                Item            Function        To change the radio station, tap a preset but-
                          Increases the radio station   ton.
                          frequency. Touch and hold
                          this button to automatically
                          seek the next available ra-  Bluetooth screen
                          dio station.          Smartphones and other external devices that
           Source         Displays the media screen.  are compatible with Bluetooth can be con-
                                                nected wirelessly to the audio system to lis-
                                                ten to the audio tracks stored on the devices
           To change the radio station frequency:
                                                through the audio system’s speakers.
           Tap “   ” or “  ” to tune to a receivable
           frequency.
                                                         Bluetooth
           To save a radio station frequency to a preset
                                                              Best Of You
           button:                                            Foo Fighters
           Tune the radio to the desired radio station,       In Your Honor
           and then touch and hold the desired preset
           button for several seconds.

                            1                      Source           MPH    Zone Control
                    AM Radio      AM-1
                1    2    3    4    5
                 1710
                                                     Item            Function
                            P1                                 Displays the external de-
                                                               vice management screen.
                        1710 kHz
                                                               Displays information about
                                                               the current audio track.
              Source           MPH    Zone Control
           1  Preset button
                                                To connect an external device:
           Weather screen                       (1) Tap the “  ” button, and then select
           You can receive a weather broadcast.    “+Add Device”.
                                                (2) Turn on the Bluetooth function of the ex-
                                                   ternal  device, and  then search for the
                     NOAA National Weather
                                                   multi-function display unit of the boat.
                                                TIP:
                     CH 1 -0.000  kHz           Make sure that other external devices have
                                                their Bluetooth function disabled before be-
                1   2   3   4   5   6   7
                                                ginning the pairing  process  to reduce  con-
                                                nection issues.
              Source           MPH    Zone Control

                                                                                 61

| 64 65 66 67 68 69 70 71 72 73 74 |