Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 95 - LIT-18626-12-95
P. 95

    Instrument operation

                Item            Function        Weather screen
                          Increases the radio station   You can receive a weather broadcast.
                          frequency. Touch and hold
                          this button to automatically
                          seek the next available ra-      NOAA National Weather
                          dio station.
           Source         Displays the media screen.
                                                          CH 1 -0.000 kHz
           To change the radio station frequency:    1   2   3   4    5   6   7
           Tap “   ” or “  ” to tune to a receivable
           frequency.
                                                   Source           MPH    Zone Control
           To save a radio station frequency to a preset
           button:
           Tune the radio to the desired radio station,  To change the radio station, tap a preset but-
           and then touch and hold the desired preset  ton.
           button for several seconds.
                                                Bluetooth screen
                            1
                                                Smartphones and other external devices that
                    AM Radio      AM-1          are compatible with Bluetooth can be con-
                1    2    3    4    5
                 1710                           nected wirelessly to the audio system to lis-
                                                ten to the audio tracks stored on the devices
                            P1
                                                through the audio system’s speakers.
                        1710 kHz
                                                         Bluetooth
              Source           MPH    Zone Control            Best Of You
                                                              Foo Fighters
                                                              In Your Honor
           1  Preset button

                                                   Source           MPH    Zone Control

                                                     Item            Function
                                                               Displays the external de-
                                                               vice management screen.

                                                               Displays information about
                                                               the current audio track.

                                                                                 87

| 90 91 92 93 94 95 96 97 98 99 100 |