Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 109 - LIT-18626-12-95
P. 109

    Equipment operation

           Passenger’s seat
                                                    WARNING
           The passenger’s seat can be adjusted in the
           same ways as the driver’s seat.      Do  not sit on the swim  platform seats
           See “Driver’s seat” for instructions on adjust-  while the  engines are  running. Exhaust
           ing the seat. However, the seat bolster of the  gases coming from underneath the swim
           passenger’s seat cannot be adjusted.  platform contain carbon monoxide, a col-
                                                orless, odorless gas which may cause
                                                brain damage or death when inhaled.
                                1
                                                When the backrests are toward the stern, the
                                                center seat and the removable backrest can
                                                be installed.

                                                                       1

           1  Passenger’s seat                                          2

           Engine hood seat
           The position of the backrest for the engine
           hood seats  can  be changed by pulling the
           lock lever  toward the bow or toward the
                                                1  Backrest
           stern.
                                                2  Center seat
                             1
                                                The center seat can also be installed upside
                                                down to use as a beverage holder.

                                                Swim platform seat
                                                (252S / 252SE / 252SD)
                          2                     The swim platform seats are provided on the
                                                swim platform. WARNING! Do not sit on the
                                                swim platform seats while the engines are
                                                running. Exhaust gases coming from un-
           1  Backrest                          derneath the swim platform contain car-
           2  Lock lever                        bon monoxide, a colorless, odorless gas
                                                which may cause brain damage or death
           By moving the backrest toward the bow, the  when inhaled.
           seating area of the swim platform seats can
           be increased, and by moving the backrest to
           the stern, a seating space for the cabin area
           can be created.

                                                                                101

| 104 105 106 107 108 109 110 111 112 113 114 |