Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 60 - LIT-18626-12-95
P. 60

    Instrument operation

           Static bar

                                           NW      NE
                           FUEL                                 DEPTH
                   1                                                      4
                          50  %                                  0  Ft
                   2                                                      5

                   3                                                      6
                              START                          HOUSE
                              36.3  V                        11.8  V
                             Bilge  Blower            Nav    Anchor

                      Name                             Function
            1  Fuel level bar graph  Displays the amount of fuel remaining in the fuel tank. Depending
                                   on the amount of remaining fuel, the bar graph is displayed in 3
                                   colors: blue, orange, and red.
            2  Port engine tachometer  Displays the engine speed.
            3  Start battery voltage val-  Displays the start battery voltage in a numerical format.
               ue
            4  Depth level         Displays the water depth in feet or meters. Depending on the wa-
                                   ter depth, the bar graph is displayed in 3 colors: blue, orange, and
                                   red.
            5  Starboard engine ta-  Displays the engine speed.
               chometer
            6  House battery voltage   Displays the house battery voltage in a numerical format.
               value

           52

| 55 56 57 58 59 60 61 62 63 64 65 |