Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 195 - LIT-18626-12-95
P. 195

    Trouble recovery

                                      Troubleshooting
           If you have any trouble with your boat, use this section to check for the possible cause. If you
           cannot find the cause or if the procedure for replacement or repair is not described in this own-
           er’s/operator’s manual, ask your Yamaha Boat Dealer or a qualified mechanic for the proper
           service.

           Troubleshooting chart
           The  Troubleshooting chart  contains: “TROUBLE,” “POSSIBLE  CAUSE,” “REMEDY,” and
           “PAGE.”
           Check the possible cause and remedy, and also the referred page for the maintenance steps
           to solve the trouble.

             TROUBLE           POSSIBLE CAUSE                 REMEDY          PAGE
           Starter mo-  Engine shut-off   Clip on cord is not in  Install clip in engine shut-off
           tor does not   switch (252SE /   place     switch                   37
           turn over   252XE / 252SD)
                       Fuse           Burned out      Replace fuse and check wiring  196
                       Battery        Run down        Recharge                 176
                                      Poor terminal con-  Tighten as required  176
                                      nections
                                      Battery switch off  Turn on switch       37
                       Rear platform   Not latched    Latch securely           110
                       hatch
                       Starter compo-  Faulty         Have serviced by Yamaha   —
                       nent                           Boat Dealer
                       Remote control   Not in neutral posi-  Move remote control lever to   40
                       lever          tion            neutral position
                       Throttle/shift pad-  Squeezed  Release                  42
                       dle (252SD)

                                                                                187

| 190 191 192 193 194 195 196 197 198 199 200 |