Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 138 - LIT-18626-12-95
P. 138

    Equipment operation

           (5) Push the snap button and extend each  (7) While pulling the main pole down, push
              forward support pole until it is locked in  the snap button  and shorten each for-
              place.                               ward support pole until it is locked in
                                                   place to tighten the bimini top.

                                                                               1

                                          1
                                                                               2
                                          2

           1  Snap button
           2  Forward support pole              1  Forward support pole
                                                2  Snap button
           (6) Remove the  forward support  pole
              mounting knobs, and then secure the  NOTICE
              forward support poles to the forward
              support pole mounting  brackets using  z Do not exceed 72 km/h (45 mph) with the
              the mounting knobs.                 bimini top in the up position.
                                                z Be careful not to push the snap button
                                                  and extend the pole too far. Otherwise,
                                                  the lower section of the pole could fall
                                                  into the water.
                                  2
                    1
                                                Storing the bimini top in the upright
                                3               position
                                                 NOTICE
                                                Do not trailer the boat with the bimini top
           1  Forward support pole mounting knob  in the fully extended or upright position.
           2  Forward support pole              When transporting the boat, put the bimini
           3  Forward support pole mounting bracket  top in the fully collapsed position to avoid
                                                damage.

                                                To store the bimini top in the upright position:
                                                (1) While pulling the main pole down slightly,
                                                   push the snap button, and then extend

           130

| 133 134 135 136 137 138 139 140 141 142 143 |