Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 116 - LIT-18626-12-95
P. 116

    Equipment operation

           To  use the driver’s side console compart-
           ment door as the partition:
           (1) Unfold the door and guide the edge of it
              into the channel on  the enclosed head
              compartment.                                                  1

                                          1

                                          2
                                                1  Stowable table

           1  Edge
           2  Channel

           (2) To hold the door in place, hook the driv-
              er’s side console compartment door                           1
              latch to the metal tab on the front side of
              the door.
                                                1  Stowable table

                                                  Maximum weight limit:
                                          2         9 kg (20 lb)
                                                To stow the stowable table, lift the table and
                                                place it in its original position.

                1                               Glove compartment
                                                The glove compartment is located in front of
           1  Driver’s side console compartment door latch  the passenger’s seat.
           2  Metal tab                         To open the glove compartment:
                                                While pulling the glove compartment latch,
           Stowable table                       pull the glove compartment lid to open it.
           The stowable table is located in front of the
           passenger’s seat.
           To use the stowable table, pull the table and
           lower it until it contacts the stoppers.

           108

| 111 112 113 114 115 116 117 118 119 120 121 |