Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 111 - LIT-18626-12-95
P. 111

    Equipment operation

                     Engine hood                     Storage compartments
           The engine hood can be opened to access  This boat is equipped with the following con-
           the engines.                         venient on-board storage compartments.
           The engine hood latch is located under the  Make sure  that the storage  compartments
           front of each engine hood seat.      are securely closed before getting underway.
           To prevent excess water from spilling onto
           the engines after a rainfall or washing down  Anchor storage compartment
           the boat, wipe off the seat cushions before  The anchor storage compartment is located
           opening the engine hood.             at the bow.
           To open the engine hood, pull the engine  To open the anchor storage compartment:
           hood latch up and lift the engine hood.  Pull the anchor storage compartment lid latch
                                                to open the lid.

                                                                               1

             1                                      2

                                       2
           1  Engine hood
           2  Engine hood latch                 1  Anchor storage compartment lid
                                                2  Anchor storage compartment lid latch
           To close the engine hood, push the front of
           each engine hood seat down to securely lock
           it in place.

                                                                            1

                                                1  Anchor storage compartment
                                                When storing the anchor, place some cush-
                                                ioning material or the anchor line under the
                                                anchor.

                                                                                103

| 106 107 108 109 110 111 112 113 114 115 116 |