Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 133 - LIT-18626-12-95
P. 133

    Equipment operation

           (5) Push the snap button and extend each  (7) While pulling the main pole down, push
              rear support pole to the long position.  the snap button and shorten each rear
                                                   support pole to either the middle position
                                                   for cruising or to the short position if you
                 1                                 are using the wakeboard tower. Be sure
                 2                                 the snap buttons click into place.
                 3
                 4                                   1
                 5
                                                     2

                                                     3
           1  Rear support pole                      4
           2  Snap button
           3  Short position
           4  Middle position
           5  Long position
                                                1  Rear support pole
                                                2  Short position
           (6) Secure each rear support pole to the rear
                                                3  Middle position
              support pole mounting bracket using the  4  Snap button
              lock pin.
                                                 NOTICE
                                     1
                                                z Do not exceed 72 km/h (45 mph) with the
                                                  bimini top in the up position.
                         2         3            z Be careful not to push the snap button
                                                  and extend the pole too far. Otherwise,
                                                  the lower section of the pole could fall
                                                  into the water.

           1  Rear support pole
           2  Lock pin
           3  Rear support pole mounting bracket

                                                                                125

| 128 129 130 131 132 133 134 135 136 137 138 |