Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 194 - LIT-18626-12-95
P. 194

    Specifications

                           Item                             Specification
           Drive unit
           Propulsion system                    Jet pump
           Jet pump type                        Axial flow, single stage
           Impeller rotation                    Counterclockwise
           Pitch angle                          14.7°
           Transmission                         Direct drive from engine
           Jet thrust nozzle angle              23+23°
           Fuel and oil
           Recommended fuel                     Regular unleaded gasoline
           Minimum octane rating (PON)          86
           Minimum octane rating (RON)          90
           Fuel tank total capacity             284 L (75.0 US gal, 62.5 Imp.gal)
           Recommended engine oil               YAMALUBE 4W or 4-stroke motor oil

           Recommended engine oil type SAE      SAE 10W-30, 10W-40, 20W-40, 20W-50
           Recommended engine oil grade API     3-star models
                                                API SG, SH, SJ, SL
                                                4-star models
                                                API SJ, SL
           Engine oil total quantity            5.3 L (5.60 US qt, 4.66 Imp.qt)
           Engine oil quantity without oil filter replacement  3.5 L (3.70 US qt, 3.08 Imp.qt)
           Engine oil quantity with oil filter replacement  3.7 L (3.91 US qt, 3.26 Imp.qt)
           Fuse amperage
           Electronic throttle valve fuse       10 A
           Fuel pump fuse                       10 A
           Main relay drive fuse                10 A
           Main fuse                            20 A
           Battery fuse                         30 A
           BCU fuse (252SE / 252XE / 252SD)     50 A
           Display/Buzzer/GPS/Audio Controller/Switch
           Panel fuse                           20 A
           CLH/CLG/Power Port/USB fuse          20 A
           Horn fuse                            7.5 A
           Bilge pump fuse                      3 A
           Power distribution module fuse       20 A
           USB fuse                             3 A
           Accessory fuse                       20 A

           186

| 189 190 191 192 193 194 195 196 197 198 199 |