Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 141 - LIT-18626-12-95
P. 141

    Equipment operation

           Removing the bimini top
           To remove the bimini top:
           (1) Store the bimini top. See “Storing the bi-
              mini top in the fully collapsed position”.
           (2) Remove the main pole mounting knobs
              securing the bimini top to the main pole
              mounting brackets.

                                  1

           1  Main pole mounting knob

           (3) Remove the bimini top from the boat.

           Installing the bimini top
           To install the bimini top:
           When installing the bimini top, simply reverse
           the removal steps, and then make sure that
           the main pole mounting knobs are securely
           installed.

                                                                                133

| 136 137 138 139 140 141 142 143 144 145 146 |