Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 159 - LIT-18626-12-95
P. 159

    Pre-operation checks

                                                252SE / 252SD

                      NW    N     NE
             FUEL                        DEPTH
             50  %       FLOAT MODE       0  Ft
                                °F
                         Water Temp
               START                    HOUSE
               36.3  V                  11.8  V
                                                                   1
               Bilge  Blower        Nav  Anchor
                                    1   2
           1  “Navigation” light button
           2  “Anchor” light button             1  “NAV LIGHTS” switch
                                                Horn check
           TIP:
                                                Push the “HORN” switch and check that the
           You can also tap the navigation light indicator
                                                horn sounds.
           and the anchor light indicator on the status
                                                The switch light comes on while the horn is
           indicator bar to turn the bow light and anchor
                                                operating.
           light on or off.
                                                AR250 / SX250
           252S / 252SE / 252SD
           To check the operation using the switch pan-  1
           el:
           Push the “NAV LIGHTS” switch. Check that             HORN  BILGE
           only the anchor light or both the anchor light
           and bow light come on when the switch light
           comes on and that both lights go off when the
           switch light is off.
           252S
                                                1  “HORN” switch

                              1

           1  “NAV LIGHTS” switch

                                                                                151

| 154 155 156 157 158 159 160 161 162 163 164 |