Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 137 - LIT-18626-12-95
P. 137

    Equipment operation

                  Bimini top (SX250)            (3) Remove the storage cover, unfold the bi-
           Setting up the bimini top               mini top, and pull it toward the bow.
           To set up the bimini top:
           (1) Raise the  bimini top,  and then remove
              the lock pins securing the rear support         1
              poles to the main pole.

                              1
                                                1  Storage cover

                                                (4) Unhook the forward support poles from
                                                   the main pole.
           1  Rear support pole
           (2) Secure each rear support pole to the rear
              support pole mounting bracket using the                          2
              lock pin. Make sure that the tab on the
              end of the lock pin is pointing downward.           1

              1

                                                1  Forward support pole
                                                2  Main pole
                  2

                               3

           1  Rear support pole
           2  Rear support pole mounting bracket
           3  Lock pin

                                                                                129

| 132 133 134 135 136 137 138 139 140 141 142 |