Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 68 - LIT-18626-12-95
P. 68

    Instrument operation

                     Media screen               currently connected device, and  then  con-
           This screen can be used to receive a radio  nect the other device.
           broadcast, connect to an external device us-
           ing Bluetooth wireless technology, and per-  To change the volume:
           form other functions.                The following slider is displayed in each
                                                screen.
                                                Use the slider control to change the volume.
                          Source
                                                                 1
                    AM Radio    FM Radio
                    Weather     Bluetooth
                          Auxiliary             1  Slider control

                                                TIP:
             Turn Off    Select a Source  Zone Control
                                                The volume can also be adjusted by tapping
                                                the “   ” or “  ” button.
                Item            Function
           AM Radio       Switches the source to the
                          AM radio tuner and dis-  Radio screen (AM/FM)
                          plays the AM radio screen.  You can receive a radio broadcast.
           FM Radio       Switches the source to the
                          FM radio tuner and dis-
                          plays the FM radio screen.      AM Radio      AM-1
                                                      1    2    3    4    5
           Weather        Switches the source to the   1710
                          weather radio tuner and
                          displays the weather radio              P1
                          screen.
                                                              1710 kHz
           Bluetooth      Switches the source to an
                          external device connected
                          using Bluetooth wireless
                          technology, and displays   Source          MPH   Zone Control
                          the Bluetooth screen.
           Auxiliary      Switches the source to the
                          auxiliary device and dis-  Item            Function
                          plays the auxiliary screen.
                                                               Decreases the radio sta-
           Turn Off       Turns the audio system on            tion frequency. Touch and
                          or off.                              hold this button to auto-
           Zone Control   Displays the volume ad-              matically seek the next
                          justment screen for each             available radio station.
                          zone.                                Decreases the radio sta-
                                                               tion frequency.
           TIP:
           If multiple external devices are connected at       Increases the radio station
           the same time, the audio system may not op-         frequency.
           erate properly. When switching from one ex-
           ternal device to another one, disconnect the

           60

| 63 64 65 66 67 68 69 70 71 72 73 |